README file


* After unzipping the AMS60.zip file, you should install ASMWIN 6.0 by clicking
  on the "setup.exe" icon to install it in a specified directory on your PC. (If
  you haven't already done so)

* Also unzip the files rma1.zip and donttouch.zip.  Put them in different folders marked
  /RMA1  and  /DONTTOUCH , respectively.

RMA1 folder     -->  Will have the aquifer geometry and observation pts for HW 1; 
			A series of files you can open as RMA1.ASM from within ASMWIN.
	
			you will need to fix:
			porosity, hydraulic conductivity, specified flow boundaries,
			wells (if needed), constant head boundaries, etc.


DONTTOUCH folder-->  This is a *copy* of the files in the RMA1 folder... if you mess up the 
			the model you are working on in RMA1, you will copy this folder
			and rename it to "start over".  The "save options" are primitive
			in ASMWIN, so you need to always keep this untouched copy in DONTTOUCH.
